min_slic3r_version = 2.2.0-alpha0
1.1.0 Filament aliases, Creality profiles and other goodies for PrusaSlicer 2.2.0-alpha0
min_slic3r_version = 2.1.1-beta0
1.0.6 Added Prusa MINI profiles
min_slic3r_version = 2.1.0-alpha0
1.0.5 Added SLA materials
1.0.4 Updated firmware version and 0.25mm nozzle profiles
1.0.3 Added filament profiles
1.0.2 Added SLA materials
1.0.1 Updated MK3 firmware version check to 3.8.0, new soluble support profiles for 0.6mm nozzle diameter MMU2S printers.
1.0.0 Updated end G-code for the MMU2 profiles to lift the extruder at the end of print. Wipe tower bridging distance was made smaller for soluble supports.
1.0.0-beta1 Updated color for the ASA filaments to differ from the other filaments. Single extruder printers now have no extruder color assigned, obects and toolpaths will be colored with the color of the active filament.
1.0.0-beta0 Printer model checks in start G-codes, ASA filament profiles, limits on min / max SL1 exposition times
1.0.0-alpha2 Printer model and nozzle diameter check
1.0.0-alpha1 Added Prusament ASA profile
1.0.0-alpha0 Filament specific retract for PET and similar copolymers, and for FLEX
min_slic3r_version = 1.42.0-alpha6
0.8.7 Updated firmware version
0.8.6 Updated firmware version for MK2.5/S and MK3/S
0.8.5 Updated SL1 printer and material settings
0.8.4 Added Prusament ASA profile
0.8.3 FW version and SL1 materials update
0.8.2 FFF and SL1 settings update
0.8.1 Output settings and SLA materials update
0.8.0 Updated for the PrusaSlicer 2.0.0 final release
0.8.0-rc2 Updated firmware versions for MK2.5/S and MK3/S
0.8.0-rc1 Updated SLA profiles
0.8.0-rc Updated for the PrusaSlicer 2.0.0-rc release
0.8.0-beta4 Updated SLA profiles
0.8.0-beta3 Updated SLA profiles
0.8.0-beta2 Updated SLA profiles
0.8.0-beta1 Updated SLA profiles
0.8.0-beta Updated SLA profiles
0.8.0-alpha9 Updated SLA and FFF profiles
0.8.0-alpha8 Updated SLA profiles
0.8.0-alpha7 Updated SLA profiles
0.8.0-alpha6 Updated SLA profiles
min_slic3r_version = 1.42.0-alpha
0.8.0-alpha Updated SLA profiles
0.4.0-alpha4 Updated SLA profiles
0.4.0-alpha3 Update of SLA profiles
0.4.0-alpha2 First SLA profiles
min_slic3r_version = 1.41.3-alpha
0.4.10 Updated firmware version
0.4.9 Updated firmware version for MK2.5/S and MK3/S
0.4.8 MK2.5/3/S FW update
0.4.7 MK2/S/MMU FW update
0.4.6 Updated firmware versions for MK2.5/S and MK3/S
0.4.5 Enabled remaining time support for MK2/S/MMU1
0.4.4 Changelog: https://github.com/prusa3d/Slic3r-settings/blob/master/live/PrusaResearch/changelog.txt
0.4.3 Changelog: https://github.com/prusa3d/Slic3r-settings/blob/master/live/PrusaResearch/changelog.txt
0.4.2 Changelog: https://github.com/prusa3d/Slic3r-settings/blob/master/live/PrusaResearch/changelog.txt
0.4.1 New MK2.5S and MK3S FW versions
0.4.0 Changelog: https://github.com/prusa3d/Slic3r-settings/blob/master/live/PrusaResearch/changelog.txt 
min_slic3r_version = 1.41.1
0.3.10 Updated firmware version
0.3.9 Updated firmware version for MK2.5/S and MK3/S
0.3.8 MK2.5/3/S FW update
0.3.7 MK2/S/MMU FW update
0.3.6 Updated firmware versions for MK2.5 and MK3
0.3.5 New MK2.5 and MK3 FW versions
0.3.4 Changelog: https://github.com/prusa3d/Slic3r-settings/blob/master/live/PrusaResearch/changelog.txt 
0.3.3 Prusament PETG released
0.3.2 New MK2.5 and MK3 FW versions
0.3.1 New MK2.5 and MK3 FW versions
0.3.0 New MK2.5 and MK3 FW version
min_slic3r_version = 1.41.0-alpha
0.2.9 New MK2.5 and MK3 FW versions
0.2.8 New MK2.5 and MK3 FW version
min_slic3r_version = 1.41.1
0.2.7 New MK2.5 and MK3 FW version
0.2.6 Added MMU2 MK2.5 settings
min_slic3r_version = 1.41.0-alpha
0.2.5 Prusament is out - added prusament settings
0.2.4 Added soluble support profiles for MMU2
0.2.3 Added materials for MMU2 single mode, edited MK3 xy stealth feedrate limit
0.2.2 Edited MMU2 Single mode purge line
0.2.1 Added PET and BVOH settings for MMU2
0.2.0-beta5 Fixed MMU1 ramming parameters
0.2.0-beta4 Added filament loading speed at start, increased minimal purge on wipe tower
0.2.0-beta3 Edited ramming parameters and filament cooling moves for MMU2
0.2.0-beta2 Edited first layer speed and wipe tower position
0.2.0-beta Removed limit on the MK3MMU2 height, added legacy M204 S T format to the MK2 profiles
0.2.0-alpha8 Added filament_load/unload_time for the PLA/ABS MMU2 filament presets.
0.2.0-alpha7 Vojtech's fix the incorrect *MK3* references
0.2.0-alpha6 Jindra's way to fix the 0.2.0-alpha5 version
0.2.0-alpha5 Bumped up firmware versions for MK2.5/MK3 to 3.3.1, disabled priming areas for MK3MMU2
0.2.0-alpha4 Extended the custom start/end G-codes of the MMU2.0 printers for no priming towers.
0.2.0-alpha3 Adjusted machine limits for time estimates, added filament density and cost
0.2.0-alpha2 Renamed the key MK3SMMU to MK3MMU2, added a generic PLA MMU2 material
0.2.0-alpha1 added initial profiles for the i3 MK3 Multi Material Upgrade 2.0
0.2.0-alpha moved machine limits from the start G-code to the new print profile parameters
min_slic3r_version = 1.40.0
0.1.18 Updated firmware version
0.1.17 Updated firmware version for MK2.5/S and MK3/S
0.1.16 MK2.5/3/S FW update
0.1.15 MK2/S/MMU FW update
0.1.14 Updated firmware versions for MK2.5 and MK3
0.1.13 New MK2.5 and MK3 FW versions
0.1.12 New MK2.5 and MK3 FW versions
0.1.11 fw version changed to 3.3.1
0.1.10 MK3 jerk and acceleration update
0.1.9 edited support extrusion width for 0.25 and 0.6 nozzles
0.1.8 extrusion width for 0,25, 0.6 and variable layer height fixes
0.1.7 Fixed errors in 0.25mm and 0.6mm profiles
0.1.6 Split the MK2.5 profile from the MK2S
min_slic3r_version = 1.40.0-beta
0.1.5 fixed printer_variant fields for the i3 MK3 0.25 and 0.6mm nozzles
0.1.4 edited fw version, added z-raise after print
min_slic3r_version = 1.40.0-alpha
0.1.3 Fixed an incorrect position of the max_print_height parameter
0.1.2 Wipe tower changes
0.1.1 Minor print speed adjustments
0.1.0 Initial
